
                         Manual for Update of JBT-CS Scanner <220>
    Before your update, please read our manual of update carefully. If you also have any 
questions, please to contact service center of Beijing Jinbenteng Auto S&T Co., Ltd.
Contacts:
        Address:   Building32, Block 11, No. 188, South 4th Ring Road, Fengtai District,
                   Beijing, China.
        Postcode:  100070
        Telephone: (TEL:+86 /10/ 52220868)

A.   Introduction for software interface
  1. In the interface, there is letter with underline in brackets at the behind of every
     text string, which is shortcut key for users to choose this item. Details:press Alt
     key first, and then choose letters at the behind of the text strings for every fun-
     -ction.
  2. Bill of "Choose serial port" is for us to choose the serial port, and this software
     can match the serial port automatically,if we connect the USB with PC and open this
     software. Once the serial port is taken by other equipment, the scanner can not be 
     connected with PC. If so, we can move the equipment or change to other serial port.
  3. Bill of "Operation for Scanner" is for you to operate the scanner:
    3.1 Bill of "update and verify" is to update and verify the program and data for sc-
        -anner, which is the same to choose "update" first, and then "verify". The time 
        for "update and verify" is longer than the time for "update" and "verify" separ-
        -ately.
    3.2 "Update" is to update the program and data for "CS" Scanner. After update, the  
        scanner is with the latest software for this model and with the latest testing  
        functions.
    3.3 "Verify" is to verify the program and data after update. If there is any error, 
        we must update it again. The function for "verify" is to check the program and  
        data of update for the scanner.
  4. You input the name of update software ( extension-named as *.BIN) to "file for ope-
     -ration", which can be downloaded from the website of Beijing Jingbenteng Auto S&T 
     Co., ltd. (WWW.JINBENTENG.COM). You can either input name of file directly,or click 
     "browse" and choose the update file. Please do it step by step according to "opera-
     -tion prompt"
  5. In this content, there is one base platform system update file named CSSYS.BIN, wh-
     -ich is to drive system of base platform. For example: the font library for "CS" 
     scanner is damaged, the load of basic function is with error, or some others. Users
     all need to update CSSYS.BIN.The details: You can input CSSYS.BIN directly to "file
     for operation" ( or click ¡°browse¡± and choose CSSYS.BIN), and then click "Start" 
     to update  base platform for "CS" Scanner.
  6. Button function introduction: "browse" button is used to select the operated file, 
     "start" button is to start the communication link between computer and scanner. "S-
     -top" button is used to stop the communication link between computer and scanner.  
     "Close" is used to close the application.
  7. "Operation caution": used to prompt synchronously the current operation status and 
     instruct the end-user to operate,"current module" shows function module title which
     is being operated, "connection status" shows the current data communication direct-
     -ion, "speed proportion" indicates the operation schedule.
  8. "Page speed gene" is used to define the communication speed when starting to page  
     "CS" scanner, the gene's value scope: 150-300, the initial default value is 180, 
     the bigger the value is, the longer the paging interval is. "Communication speed g-
     -ene" is used to set the communication speed between computers and auto scanner,the
     gene's value scope is 0-200,the initial default value is 20, the smaller the value 
     is, the communication speed between computer and scanner is bigger. Generally spea-
     -king, the smaller the value of the two gene is, the bigger the communication speed
     is; the bigger the value is, the more stable the communication performance is. The-
     -refore, the speed and performance could reach the best condition by adjust the two
     speed gene according to different computer hardware performance. Setting method, by
     using keyboard(press Alt+H/Alt+T, select respective speed gene horizontal, do the  
     size adjustment by left-right arrow), by using mouse(to click directly the respect-
     -ive speed gene horizontal scroll bar's left-right arrow to do the size adjustment). 
     Each operation, the application will remember the speed gene value the end-user set 
     last time.
B.   Operation steps for JBT auto scanner "update + verify", "update" and "verify"
  1. Download the updating software from JBT company website: www.jinbenteng.com
  2. Connect the computer with auto scanner by the USB cable (JBT USB appointed cable). 
     If your computer hasn¡¯t set up the USD drive software, please do not make the auto 
     scanner power on. Please get the USB drive software from JBT website. 
  3. Run "JBT "CS" auto scanner special updating program<V2.8>"
  4. From the menu "for auto scanner operation", please choose the function you need.
  5. According to the tips in the "operation notice", input the name of update document. 
     (Generally you can choose by ¡°browse¡±). Press ¡°Start¡±, and connect with CS auto 
     scanner. The computer will communicate with CS auto scanner automatically after the 
     auto scanner is powered on. Then finish the operation as appointed.


                                                                     March 25, 2011 